Ryan Young

CSE 2300W

Lab 2

Question 1.

We are using the 7405 invertor instead of the 7404 because we need to drive an external load.

Question 2.

The current going through each LED is 0.00376 amps because they are in series with a 1000 Ohm resitor and a 330 Ohm resistor.